*Question G1C02:
[97.313] What is the maximum transmitter power an amateur station may use on the 12-meter band?*  

*Correct Answer is  C: 1500 watts PEP output*  

### AI Response: (may contain errors)  

In the context of amateur radio, the term "PEP" stands for Peak Envelope Power, which is the maximum power level of a signal during a single RF cycle. The FCC regulations specify the maximum power levels that can be used on different amateur bands.

1. **Correct Answer Explanation:**
   - The correct answer is **C: 1500 watts PEP output**. According to FCC Part 97.313, the maximum transmitter power for most amateur bands, including the 12-meter band, is 1500 watts PEP output. This is the highest power level allowed for amateur stations to ensure efficient communication while minimizing interference.

2. **Incorrect Answers Explanation:**
   - **A: 50 watts PEP output**: This is incorrect because 50 watts is below the maximum allowed power. While some bands or specific modes might have lower power limits, the 12-meter band allows up to 1500 watts PEP.
   - **B: 200 watts PEP output**: This is also incorrect for the same reason as above. 200 watts is below the maximum allowed power for the 12-meter band.
   - **D: An effective radiated power equivalent to 100 watts from a half-wave dipole**: This is incorrect because it refers to effective radiated power (ERP), which is not the same as PEP output. The 12-meter band regulation specifies PEP output, not ERP.

3. **Useful Rule of Thumb:**
   - For most HF bands, including the 12-meter band, the maximum power limit is 1500 watts PEP output unless otherwise specified by specific band plans or international agreements. Always check the specific band plan for any exceptions or additional restrictions.