*Question G1C05:
[97.313] What is the limit for transmitter power on the 28 MHz band for a General Class control operator?*  

*Correct Answer is  C: 1500 watts PEP output*  

### AI Response: (may contain errors)  

The correct answer is C: 1500 watts PEP output.

1. **Why the correct answer is correct:**
   - According to FCC regulations, the maximum transmitter power for a General Class control operator on the 28 MHz band (which is part of the 10-meter amateur radio band) is 1500 watts PEP (Peak Envelope Power) output. This is the standard maximum power limit for most amateur bands unless otherwise specified.

2. **Why the other choices are incorrect:**
   - **A: 100 watts PEP output**: This is incorrect because 100 watts is below the maximum allowed power. While some bands or modes may have lower power limits, the 28 MHz band allows up to 1500 watts for General Class operators.
   - **B: 1000 watts PEP output**: This is incorrect because it is also below the maximum allowed power. Although 1000 watts is a common power level for many amateur radio amplifiers, the legal limit is 1500 watts.
   - **D: 2000 watts PEP output**: This is incorrect because it exceeds the maximum legal limit. The FCC restricts the maximum power to 1500 watts PEP to minimize interference and ensure fair use of the spectrum.

3. **Useful rules of thumb:**
   - **PEP (Peak Envelope Power)** is the maximum power level during a single RF cycle at the crest of the modulation envelope. It is the standard measurement for power limits in amateur radio.
   - Always check the specific band and license class for any exceptions to the general 1500 watts PEP limit, as some bands have lower limits or additional restrictions.