*Question G1C05:
[97.313] What is the limit for transmitter power on the 28 MHz band for a General Class control operator?*  

*Correct Answer is  C: 1500 watts PEP output*  

### AI Response: (may contain errors)  

The correct answer to the question about the limit for transmitter power on the 28 MHz band for a General Class control operator is:

**C: 1500 watts PEP output**

### Explanation:

1. **Why the correct answer is correct:**
   - According to the FCC regulations, General Class licensees are allowed to operate with a maximum power output of 1500 watts PEP (Peak Envelope Power) on the 28 MHz band. This limit is set to ensure efficient use of the spectrum while minimizing interference with other users.

2. **Why the other choices are incorrect:**
   - **A: 100 watts PEP output**: This limit applies to Technician Class operators on certain bands, but not to General Class operators on the 28 MHz band.
   - **B: 1000 watts PEP output**: This limit is not applicable to the 28 MHz band for General Class operators. It may apply to other bands or license classes but not here.
   - **D: 2000 watts PEP output**: This exceeds the maximum allowed power for General Class operators on the 28 MHz band. Such a limit may apply to other specific situations or license classes, but not for General Class.

### Useful Rules of Thumb:
- Always refer to the latest FCC regulations for power limits associated with different bands and license classes.
- Remember that PEP is the maximum power output of the transmitter during transmission, which is crucial for understanding power limits in amateur radio.

This knowledge is essential for ensuring compliance with regulations while operating your station effectively.