*Question G2E08:
In what segment of the 20-meter band are most digital mode operations commonly found?*  

*Correct Answer is  D: Between 14.070 MHz and 14.100 MHz*  

### AI Response: (may contain errors)  

The correct answer to the question about where most digital mode operations are commonly found in the 20-meter band is:

**D: Between 14.070 MHz and 14.100 MHz.**

### Explanation of the Correct Answer:
- The segment between 14.070 MHz and 14.100 MHz is designated for digital modes, including popular modes like PSK31, RTTY, and others. This range is specifically allocated for digital communications, making it the most common area for such operations.

### Why the Other Choices are Incorrect:
- **A: At the bottom of the slow-scan TV segment, near 14.230 MHz**
  - This frequency is primarily used for slow-scan television (SSTV) and is not the main area for digital modes. SSTV is a different mode of operation that does not encompass the majority of digital communications.

- **B: At the top of the SSB phone segment, near 14.325 MHz**
  - This frequency is within the single sideband (SSB) phone segment, which is primarily used for voice communications. Digital modes do not typically operate in this area, as it is reserved for voice transmissions.

- **C: In the middle of the CW segment, near 14.100 MHz**
  - While 14.100 MHz is close to the digital segment, it is primarily used for continuous wave (CW) operations. CW is a mode of communication using Morse code, and it does not represent the digital modes that are more commonly found in the specified range.

### Summary:
- Digital modes are specifically allocated between 14.070 MHz and 14.100 MHz, making option D the correct choice. Understanding band allocations is crucial for effective operation and compliance with amateur radio regulations.