*Question G1A07:
[97.305(a)] On which amateur frequencies in the 10-meter band may stations with a General class control operator transmit CW emissions?*  

*Correct Answer is  D: The entire band*  

### AI Response: (may contain errors)  

In the 10-meter band, General class operators are allowed to transmit CW (Continuous Wave) emissions across the entire band. Here's a breakdown of the question and the reasoning behind the correct answer:

1. **Correct Answer Explanation**:
   - The entire 10-meter band for amateur radio is from 28.000 MHz to 29.700 MHz. General class operators can transmit CW emissions anywhere within this range. Therefore, the correct answer is **D: The entire band**.

2. **Why Other Choices Are Incorrect**:
   - **A: 28.000 MHz to 28.025 MHz only**: This choice is too restrictive. While CW can be transmitted in this range, it is not limited to just these frequencies.
   - **B: 28.000 MHz to 28.300 MHz only**: This choice incorrectly excludes the frequencies from 28.300 MHz to 29.700 MHz, where CW emissions are also permitted for General class operators.
   - **C: 28.025 MHz to 28.300 MHz only**: This choice is also too restrictive and ignores the lower part of the band (28.000 MHz to 28.025 MHz) and the frequencies above 28.300 MHz.

3. **Useful Rules of Thumb**:
   - Always remember that General class operators have access to the entire 10-meter band for CW emissions.
   - Familiarize yourself with the band plan and frequency allocations for different classes of licenses to avoid confusion during the exam.

In summary, General class operators can transmit CW emissions across the entire 10-meter band, making option D the correct choice.