*Question G1C04:
[97.303(i)] Which of the following is required by the FCC rules when operating in the 60-meter band?*  

*Correct Answer is  A: If you are using an antenna other than a dipole, you must keep a record of the gain of your antenna*  

### AI Response: (may contain errors)  

The correct answer to the question about operating in the 60-meter band is:

**A: If you are using an antenna other than a dipole, you must keep a record of the gain of your antenna.**

### Explanation of the Correct Answer:
- The FCC has specific rules for operating in the 60-meter band, which is a unique allocation with restrictions. One of these rules states that if you are using an antenna that is not a dipole, you must document the gain of that antenna. This is important for ensuring compliance with power limits and maintaining proper operation within the band.

### Why the Other Choices are Incorrect:
- **B: You must keep a record of the date, time, frequency, power level, and stations worked.**
  - This is not a requirement for the 60-meter band specifically. While keeping logs is good practice for all amateur operations, it is not mandated by the FCC for this band.

- **C: You must keep a record of all third-party traffic.**
  - This is not a specific requirement for the 60-meter band. Third-party traffic regulations apply generally but do not necessitate record-keeping for every instance on this band.

- **D: You must keep a record of the manufacturer of your equipment and the antenna used.**
  - There is no requirement to document the manufacturer of your equipment or antenna for operating in the 60-meter band. The focus is on the antenna gain if it is not a dipole.

### Summary:
- The key takeaway is that the FCC requires documentation of antenna gain when using non-dipole antennas in the 60-meter band to ensure compliance with operational limits. Other choices do not reflect specific FCC requirements for this band. 

This understanding is crucial for passing the Extra Class exam and for responsible operation in the amateur radio service.