*Question T8B12:
Which of the following is a way to determine whether your satellite uplink power is neither too low nor too high?*  

*Correct Answer is  C: Your signal strength on the downlink should be about the same as the beacon*  

### AI Response: (may contain errors)  

To determine whether your satellite uplink power is neither too low nor too high, the correct answer is:

**C: Your signal strength on the downlink should be about the same as the beacon.**

### Explanation of the Correct Answer:
- **Signal Strength Comparison**: The beacon signal from the satellite is a known reference. If your downlink signal strength is approximately the same as the beacon, it indicates that your uplink power is at an appropriate level. This means you are transmitting enough power to reach the satellite without overloading it.

### Explanation of the Incorrect Choices:
- **A: Check your signal strength report in the telemetry data**  
  - **Why it's incorrect**: While telemetry data can provide useful information about your signal, it may not directly indicate whether your uplink power is optimal. It can show if the signal is received, but it doesn't specifically compare it to a known reference like the beacon.

- **B: Listen for distortion on your downlink signal**  
  - **Why it's incorrect**: Distortion can indicate that your signal is too strong (overdriving the receiver) or too weak (poor quality). However, it does not provide a clear measure of whether your uplink power is at the correct level. Distortion is a symptom rather than a definitive measure.

- **D: All these choices are correct**  
  - **Why it's incorrect**: Since options A and B do not provide a reliable method for determining optimal uplink power, this choice cannot be correct.

### Useful Rules of Thumb:
- **Signal Strength**: Aim for your downlink signal strength to match the beacon level. This is a good practice for ensuring your uplink power is set correctly.
- **Monitoring Distortion**: If you hear distortion, consider reducing your uplink power to avoid overloading the satellite's receiver.

By focusing on the beacon comparison, you can effectively manage your uplink power for optimal satellite communication.