*Question G2E15:
Which of the following is a common location for FT8?*  

*Correct Answer is  C: Approximately 14.074 MHz to 14.077 MHz*  

### AI Response: (may contain errors)  

FT8 is a digital mode used in amateur radio that operates within specific frequency ranges. 

1. **Why the correct answer is correct:**
   - FT8 is commonly used in the 20-meter band, specifically between approximately 14.074 MHz and 14.077 MHz. This range is designated for digital modes, making it a popular choice for FT8 operations. The frequency range allows for effective communication using this mode, which is designed for weak signal conditions.

2. **Why the other choices are incorrect:**
   - **A: Anywhere in the voice portion of the band**  
     This is incorrect because FT8 is not used in the voice portion of the band, which is typically reserved for SSB (Single Sideband) voice communications.
   
   - **B: Anywhere in the CW portion of the band**  
     This is also incorrect as FT8 does not operate in the CW (Continuous Wave) portion of the band, which is reserved for Morse code transmissions.
   
   - **D: Approximately 14.110 MHz to 14.113 MHz**  
     This range is not commonly used for FT8. Instead, it is often used for other digital modes or voice communications, but not specifically for FT8.

3. **Useful rules of thumb:**
   - Digital modes like FT8 are typically found in designated segments of the HF bands, often just above the CW portions and below the voice portions.
   - Always check band plans and operating guidelines for your specific region to ensure compliance with frequency usage.

In summary, the correct frequency range for FT8 is approximately 14.074 MHz to 14.077 MHz, making it essential to know this for effective operation and exam preparation.