*Question G1C06:
[97.313] What is the limit for transmitter power on the 1.8 MHz band?*  

*Correct Answer is  D: 1500 watts PEP output*  

### AI Response: (may contain errors)  

The correct answer to the question about the limit for transmitter power on the 1.8 MHz band is:

**D: 1500 watts PEP output**

### Explanation:

1. **Why the correct answer is correct:**
   - The 1.8 MHz band, which falls within the 160-meter amateur radio band, has a maximum power limit of 1500 watts PEP (Peak Envelope Power) output. This limit is set by the FCC regulations for amateur radio operators to ensure fair use of the spectrum and to minimize interference with other services.

2. **Why the other choices are incorrect:**
   - **A: 200 watts PEP output**: This is incorrect because it is significantly lower than the actual limit for the 1.8 MHz band.
   - **B: 1000 watts PEP output**: While this is a common limit for some other bands, it is still below the maximum allowed for the 1.8 MHz band.
   - **C: 1200 watts PEP output**: This is also incorrect as it does not meet the maximum limit of 1500 watts for this band.

### Useful Rules of Thumb:
- Always refer to the latest FCC regulations or the ARRL band plan for the most accurate and up-to-date power limits for each amateur band.
- Remember that the maximum power output is typically expressed in PEP, which is the maximum power level of the transmitted signal during its peak.

This information is crucial for understanding the operational limits of the 1.8 MHz band and ensuring compliance with amateur radio regulations.