*Question E1D08:
[97.207] Which VHF amateur bands have frequencies authorized for space stations?*  

*Correct Answer is  D: 2 meters*  

### AI Response: (may contain errors)  

The correct answer to the question about which VHF amateur bands have frequencies authorized for space stations is:

**Correct Answer: D: 2 meters**

### Explanation:

1. **Why the correct answer is correct:**
   - The 2-meter band (144-148 MHz) is specifically authorized for use by amateur radio operators for communication with space stations, including satellites. This band is widely used for satellite communications due to its favorable propagation characteristics and the availability of equipment.

2. **Why the other choices are incorrect:**
   - **A: 6 meters and 2 meters**: While the 2-meter band is correct, the 6-meter band (50-54 MHz) is not typically used for space station communications.
   - **B: 6 meters, 2 meters, and 1.25 meters**: This option includes both the 6-meter and 1.25-meter bands (222-225 MHz), neither of which are primarily used for space station communications. Only the 2-meter band is authorized.
   - **C: 2 meters and 1.25 meters**: Again, while the 2-meter band is correct, the 1.25-meter band is not authorized for space station communications.

### Useful Rules of Thumb:
- The 2-meter band is the primary band for satellite communications in amateur radio.
- Always refer to the latest FCC regulations and band plans for specific frequency allocations and authorized uses.

This information is crucial for understanding the operational parameters of amateur radio, especially in the context of space communications.