*Question G2E11:
What is the primary purpose of an Amateur Radio Emergency Data Network (AREDN) mesh network?*  

*Correct Answer is  C: To provide high-speed data services during an emergency or community event*  

### AI Response: (may contain errors)  

The primary purpose of an Amateur Radio Emergency Data Network (AREDN) mesh network is to provide high-speed data services during an emergency or community event. Let's break down why this is the correct answer and why the other options are not suitable.

### Correct Answer: C
- **High-Speed Data Services**: AREDN is designed to facilitate communication and data transfer in situations where traditional infrastructure may be compromised. This includes providing services like email, file sharing, and other data applications that can be crucial during emergencies.

### Why the Other Choices are Incorrect:
- **A: To provide FM repeater coverage in remote areas**  
  - While FM repeaters are important for voice communication, AREDN specifically focuses on data services rather than extending voice coverage. Its primary function is not to enhance FM repeater systems.

- **B: To provide real-time propagation data by monitoring amateur radio transmissions worldwide**  
  - AREDN does not primarily serve as a propagation monitoring tool. Instead, it is focused on creating a robust data network for emergency communications, rather than gathering propagation data.

- **D: To provide DX spotting reports to aid contesters and DXers**  
  - DX spotting reports are typically used for enhancing HF operations and contesting. AREDN is not designed for this purpose; it is more about establishing reliable data communication networks during emergencies.

### Summary
AREDN mesh networks are essential for providing high-speed data services in emergencies, making them a vital tool for amateur radio operators in crisis situations. Understanding the specific functions of AREDN helps clarify its role compared to other amateur radio services.