*Question E1C07:
[97.303(g)] What notifications must be given before transmitting on the 630- or 2200-meter bands?*  

*Correct Answer is  D: Operators must inform the Utilities Technology Council (UTC) of their call sign and coordinates of the station*  

### AI Response: (may contain errors)  

To understand the requirements for transmitting on the 630- or 2200-meter bands, let's break down the correct answer and the other options.

### Correct Answer: 
**D: Operators must inform the Utilities Technology Council (UTC) of their call sign and coordinates of the station.**

- **Explanation**: Before operating on these bands, which are primarily used for experimental and low-frequency communications, operators are required to notify the UTC. This is to ensure that the operation does not interfere with utility operations, as these frequencies can affect power line communications and other utility services.

### Why the Other Choices are Incorrect:

- **A: A special endorsement must be requested from the FCC**  
  - **Explanation**: There is no requirement for a special endorsement from the FCC specifically for operating on the 630- or 2200-meter bands. Operators must hold an Extra Class license to use these bands, but no additional endorsement is needed.

- **B: An environmental impact statement must be filed with the Department of the Interior**  
  - **Explanation**: While environmental considerations are important, there is no requirement for amateur radio operators to file an environmental impact statement with the Department of the Interior before operating on these bands.

- **C: Operators must inform the FAA of their intent to operate, giving their call sign and distance to the nearest runway**  
  - **Explanation**: This requirement is not applicable to amateur radio operations on the 630- or 2200-meter bands. The FAA is concerned with aviation safety, but the notification to the UTC is the specific requirement for these bands.

### Summary:
- **Key Requirement**: Notify the UTC with your call sign and station coordinates before transmitting on the 630- or 2200-meter bands.
- **No special endorsements or environmental statements are required** for amateur radio operators on these frequencies.

This understanding is crucial for compliance and safe operation within the amateur radio spectrum.