*Question T1F05:
[97.119(b)(2)] What method of call sign identification is required for a station transmitting phone signals?*  

*Correct Answer is  B: Send the call sign using a CW or phone emission*  

### AI Response: (may contain errors)  

To identify your station when transmitting phone signals, the correct method is to send your call sign using a CW (Continuous Wave) or phone emission. This is important for compliance with FCC regulations.

### Explanation of the Correct Answer:
- **Correct Answer: B: Send the call sign using a CW or phone emission**  
  This option is correct because the FCC requires that all amateur radio operators identify their station using their call sign. This can be done in either CW (Morse code) or voice (phone) modes. This ensures that other operators can identify the source of the transmission.

### Explanation of Incorrect Answers:
- **A: Send the call sign followed by the indicator RPT**  
  This is incorrect because the "RPT" indicator is used for repeaters, not for general identification of a station. It does not apply to standard phone transmissions.

- **C: Send the call sign followed by the indicator R**  
  This is also incorrect. The "R" indicator is not a standard requirement for identifying a station in phone transmissions. It is not recognized as a valid method of identification.

- **D: Send the call sign using only a phone emission**  
  This is incorrect because it implies that you can only use phone emissions. While you can use phone emissions, the rule allows for identification using either CW or phone, making this option too restrictive.

### Key Points:
- Always identify your station with your call sign.
- Identification can be done in either CW or phone modes.
- Familiarize yourself with the specific indicators and their appropriate contexts to avoid confusion.

This understanding will help you correctly identify your station and comply with FCC regulations during your amateur radio operations.