*Question E1C07:
[97.303(g)] What notifications must be given before transmitting on the 630- or 2200-meter bands?*  

*Correct Answer is  D: Operators must inform the Utilities Technology Council (UTC) of their call sign and coordinates of the station*  

### AI Response: (may contain errors)  

To operate on the 630-meter or 2200-meter bands, amateur radio operators must notify the Utilities Technology Council (UTC) of their call sign and the coordinates of their station. This is to ensure that there is no interference with power line communication systems that operate in the same frequency range.

### Explanation:

1. **Correct Answer (D):**  
   - **Utilities Technology Council (UTC) Notification:**  
     - The UTC manages the coordination of amateur radio operations on these bands to prevent interference with power line communication systems.  
     - Operators must provide their call sign and station coordinates to the UTC before transmitting.

2. **Incorrect Answers:**
   - **A: Special endorsement from the FCC:**  
     - No special endorsement from the FCC is required to operate on these bands. The notification to the UTC is sufficient.
   - **B: Environmental impact statement:**  
     - An environmental impact statement is not required for amateur radio operations on these bands.
   - **C: Informing the FAA:**  
     - The FAA does not need to be informed about operations on these bands, as they are not related to aviation safety or operations.

### Key Points:
- **Notification Requirement:**  
  - The primary requirement is to notify the UTC, not to seek permission or file additional paperwork with other agencies.
- **Purpose:**  
  - This notification helps prevent interference with existing services that use similar frequencies.

Understanding these requirements ensures compliance with FCC regulations and helps maintain harmonious use of the radio spectrum.