*Question G1A04:
[97.303(h)] Which of the following amateur bands is restricted to communication only on specific channels, rather than frequency ranges?*  

*Correct Answer is  D: 60 meters*  

### AI Response: (may contain errors)  

In the context of amateur radio, certain bands have specific regulations regarding how they can be used. Let's break down the options:

1. **60 meters (Correct Answer)**:  
   - The 60-meter band is unique among amateur bands because it is restricted to communication on specific channels rather than a continuous frequency range. This means that operators must use designated frequencies (or channels) within the band, as specified by the FCC. This is done to avoid interference with other services that share the band.

2. **11 meters**:  
   - The 11-meter band is not an amateur radio band. It is allocated for Citizens Band (CB) radio, which is a different service with its own set of rules and regulations.

3. **12 meters**:  
   - The 12-meter band is part of the amateur radio HF bands and is not restricted to specific channels. Instead, it is a continuous frequency range where operators can choose their operating frequency within the band limits.

4. **30 meters**:  
   - The 30-meter band is also a continuous frequency range for amateur radio operators. It is not channelized, but it does have specific restrictions on modes and power levels to protect other services.

In summary, the 60-meter band is the only amateur band listed that is restricted to specific channels, making it the correct answer. The other options either do not apply to amateur radio or allow operation over a continuous frequency range.