*Question G1A05:
[97.301(d)] On which of the following frequencies are General class licensees prohibited from operating as control operator?*  

*Correct Answer is  A: 7.125 MHz to 7.175 MHz*  

### AI Response: (may contain errors)  

In the context of the Amateur Radio Service, different license classes have specific frequency privileges. General class licensees have certain restrictions on where they can operate.

1. **Correct Answer: 7.125 MHz to 7.175 MHz**

   - **Explanation**: This frequency range falls within the 40-meter band. According to FCC rules, General class licensees are not allowed to operate in this segment of the 40-meter band. This portion is reserved for Amateur Extra class licensees only.

2. **Why the Other Choices are Incorrect**:

   - **28.000 MHz to 28.025 MHz**: This frequency range is part of the 10-meter band. General class licensees have privileges to operate on the entire 10-meter band, so they are not prohibited from operating in this range.

   - **21.275 MHz to 21.300 MHz**: This frequency range is part of the 15-meter band. General class licensees are allowed to operate in this segment, so they are not prohibited from operating here.

3. **Useful Rules of Thumb**:

   - **General Class Privileges**: General class licensees have access to portions of most HF bands, but there are specific segments reserved for higher license classes, such as Amateur Extra.
   - **40-Meter Band**: General class licensees can operate from 7.175 MHz to 7.300 MHz, but not from 7.125 MHz to 7.175 MHz, which is reserved for Extra class.

Understanding these frequency privileges is crucial for ensuring compliance with FCC regulations and avoiding operating in restricted segments.